If BK PRECSISON 8500 was reset, the following step must be changed on the machine:

Change the budrate to 19200.

Change the trigger source to BUS

For new pc, the COM port might be different, to check the COM port use the software called “checkChipVersion\_v1006.exe”, with the correct com port the result should be “This is a PL-2303 TA chip”.