Change sys->protocol to frame

Change the budrate to 19200.

Change the trigger source to BUS

Check the PC’s COM port by Device Manager

And update the COM port in Datacollection\_window\_withfunction